Indication:

15 MS raw files

A2 to A6 should be 0 Gy

A8 to A12 should be 0.3 Gy

A14 to A18 should be 6 Gy